> Configuring DNS Settings
> Before the LDAP client can resolve names, at least one DNS server must be specified.
> Within the Dell Remote Console Switch software, the Network sub-category displays the name of the Remote Console Switch and allows you to change the network settings including the IP address, Subnet Mask, Gateway, LAN speed and DHCP/BootP setting. The name displayed for the Remote Console Switch will be the same as the name given in the System Name field in the SNMP category.
> The Network sub-category allows the entry and maintenance of up to three DNS Servers. These DNS servers are used to resolve DNS names provided on the LDAP authentication panel.

> NOTE: | At least one DNS server must be configured for the LDAP feature to work.

> NOTE: | You can also set DNS server addresses using the appliance’s serial administrative interface. For information about using the serial administrative interface, please consult your appliance documentation.

> Figure 5‑1.Network Subcategory