> Appendix C: TCP Ports
> The Video Session Viewer communicates with the 2161DS Console Switch over TCP ports 8192 and 2068. Digitized video data is sent over port TCP/UDP 8192. Encrypted keyboard and mouse data is sent over port 2068. The Appliance Management Panel (AMP) communicates with the 2161DS Console Switch over TCP/UDP port 3211. All data on ports 2068 and 3211 is encrypted using the Secure Socket Layer (SSL) protocol.
> The 2161DS Console Switch retains the database of user accounts and permissions. The Video Session Viewer performs user authentication over encrypted port 2068. The AMP performs user authentication over encrypted port 3211.
> Figure B‑1.TCP Port Communication

> NOTE: | The TCP/IP ports are fixed and cannot be altered.