> Viewing and Resynchronizing Server Connections
> When you select the Servers category for the first time, the AMP will retrieve the servers that exist in the Remote Console Switch Software database as well as information on how the servers are connected to the selected Remote Console Switch.
> The Connection column displays the current server connection. This can be to either a SIP or a tiered switch. If connected to a SIP, the SIP’s EID will display in the Connection column. If connected to a tiered switch, the switch and all of its channels will be displayed. If no unit is currently connected to the path, then this field will display as None. If you click either a SIP or switch in the Connection column, the Viewer will launch.
> Figure 4‑9.Servers Dialog Box