> Login Timeout
> In cases where there is a large enough directory tree to cause LDAP authentication to perform slowly, the Global Session panel includes a Login Timeout function with a default timeout of 30 seconds. The login timeout is the time from which the User presses the OK button on the Login Dialog until the Remote Console Switch software determines there is no response from the appliance. The appliance will also use this value to determine the timeout on a LDAP request for authentication.
> Figure 5‑6.Session panel showing Login Timeout for the Dell 2161DS

> NOTE: | This value will be stored both in the appliance and the database. When you log into the AMP, before the login is sent, the value of the timeout will be retrieved and compared to the database. If the values are different, the database will be updated to the new value. This value will be passed to the Video Viewer when a session is launched so that the Viewer can use the same login timeout.

> Figure 5‑7.Session panel showing Login Timeout for the Dell 2161DS-2 and Dell 4161DS