> Setting Up User Accounts
> When you select the Users category for the first time, the AMP will retrieve and display a list of usernames and current access levels from the Remote Console Switch. You can add, modify or delete users in this listing. You can assign three access levels: User, Administrator, and Remote Console Switch Administrator. The User access level allows you to assign individual server access rights to a user.
> Users can become locked out by the Security Lock-out feature if they try to enter an invalid password five consecutive times. You can configure Security Lock-out settings as well as unlock any user through the Users category.

> Table 4‑1.User Access Level Rights
> Operations | Remote Console Switch Administrator | Administrator | User
> Preemption | All | Equal and lesser | No
> Configure network & global settings (security mode, time-out, Simple Network Management Protocol (SNMP)) | Yes | No | No
> Reboot | Yes | No | No
> FLASH upgrade | Yes | No | No
> Administer User Accounts | Yes | Yes | No
> Monitor server status | Yes | Yes | No
> Target Device Access | Yes | Yes | Assigned by Admin

> NOTE: | Preemptions listed in Table 4-1 only apply to Remote Clients. They do not apply to users accessing the server locally.

> Figure 4‑3.Users Dialog Box
> To add or modify a user:

> 1 | Click the Users category in the left column of the AMP.

> 2 | Click the Add button on the right side of the window to add a new user. The Add User dialog box appears. -or- Select a user and click the Modify button to modify a current user. The Modify User dialog box appears.

> Figure 4‑4.Add User Dialog Box

> 3 | Type the username and password you wish to assign to the user and then verify the password by typing it in the Verify Password field.

> 4 | Select the appropriate access level you wish for this user from the drop-down list. If you select the User option, the Access Rights button becomes active.

> a | Click the Access Rights button to select individual servers for that user. The User Access Rights dialog box appears.

> Figure 4‑5.User Access Rights Dialog Box

> b | Select a server in the left column for which this user should have access rights. Click Add.

> c | Select a server in the right column from which you wish to remove the user’s access rights. Click the Remove button.

> d | Repeat steps a and b until the right column represents the appropriate server access for this user, and then click OK.

> 5 | Click OK to save the settings and return to the main AMP window.

> To change the user password:

> 1 | Select the Users category in the left column in the AMP.

> 2 | Select one user from the list and click the Modify button. The Modify User dialog appears.

> 3 | Type the password for that user in the Password box and then repeat the password in the Verify Password box. The password must be between 5 and 16 characters long and contain both alpha and numeric characters of both upper and lower case.

> 4 | Click OK to return to the AMP.

> 5 | Click Apply or OK to send the updated password to the appliance.

> To delete a user:

> 1 | Click the Users category in the left column of the AMP and then select the user(s) you wish to delete.

> 2 | Click the Delete button on the right side of the AMP U sers window. A confirmation window appears.

> 3 | Click Yes to confirm the deletion. -or- Click No to exit the window without deleting the user.