> Installing the Remote Console Switch Software
> The Remote Console Switch Software can be installed on Windows 2000, Windows 2003 Server, Windows XP and Linux platforms. Follow these instructions to install Remote Console Switch Software on the desired platform.
> To install on Windows 2000, 2003, or XP:

> 1 | Insert the Remote Console Switch Software CD-ROM into your CD-ROM drive. If AutoPlay is supported and enabled, the setup program will start automatically. -or- If your system does not support AutoPlay, set the default drive to your CD-ROM drive letter and execute the following command to start the install program (replace drive with your CD-ROM drive letter):

> drive:\WIN32\SETUP.EXE.

> 2 | Follow the on-screen instructions.

> To install on Linux:

> 1 | Insert the Remote Console Switch Software CD-ROM into your CD-ROM drive.

> 2 | If AutoMount is supported and enabled, proceed to step 3. -or- If your system does not support AutoMount:

> Mount the CD-ROM volume by executing the following command:
> mount -t iso9660 -ro mode=0555 <device> <mount point>
> Replace device with the name of the CD-ROM on your machine and mount point with the name of the desired mount point. For example, to mount a CD-ROM which is the second IDE unit on /mnt, execute the command:
> mount -t iso9660 -ro mode=0555 /dev/hdb /mnt

> 3 | At the command line, execute the following command to change the working directory to the mount point:

> cd /mnt

> 4 | Execute the following command to start the install program:

> sh ./linux/setup.bin
> Follow the on-screen instructions.