> Rebooting Your System
> You can reboot the Remote Console Switch through the Tools tab in the AMP. When clicked, Reboot will broadcast a disconnect message to any active users, then log out the current user and immediately reboot the Remote Console Switch.
> To reboot your system:

> 1 | Click the Tools tab in the AMP. The Tools dialog box appears.

> 2 | Click the Reboot button. A message prompting you to confirm this reboot appears. Click Yes to confirm the request. The Remote Console Switch will now reboot.